{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"merged":[[2,1,3,3],[4,1,8,1],[9,1,9,3],[10,1,15,1],[16,1,16,3],[17,1,24,1],[29,1,30,3],[31,1,35,1],[36,1,36,3],[37,1,43,1],[44,1,44,3],[45,1,52,1]],"flags":["formulas_cached_only"]}
[]
[]
[null,"产品介绍"]
[]
[null,"液晶屏","显示尺寸","65寸/70寸/84寸"]
[null,null,"宽度比","16:9（宽：高）",null,"  "]
[null,null,"屏类型","TFT液晶屏 LED背光"]
[null,null,"分辨率","1920*1080"]
[null,null,"对比度","5000:1（Typ.) （透射）"]
[]
[null,"触摸屏","触摸技术","非接触式红外感应技术"]
[null,null,"感应物体","不透明物体（如手指、笔等）"]
[null,null,"触摸压力","零压力"]
[null,null,"多点支持","2点、4点、10点"]
[null,null,"触摸屏玻璃","4mm，物理钢化莫氏七级防爆，透光率：>95%"]
[null,null,"操作系统支持","支持Win 7\\ Win XP \\ Win 2000\\ Linux等"]
[]
[null,"安卓方案","芯片","四核RK3188"]
[null,null,"内存","2G"]
[null,null,"内置储存","8G，可拓展"]
[null,null,"显卡","Android HD"]
[null,null,"操作系统","安卓4.2.2"]
[null,null,"内核版本","3.0.28"]
[null,null,"输入电源","220V AC 50/60HZ"]
[]
[]
[]
[]
[]
[null,"Product parameters"]
[]
[null,"LCD","Display size","65''/70''/84''"]
[null,null,"Display size","16:9 (W:H)"]
[null,null,"Screen mode"," TFT LCD, LED backlight"]
[null,null,"Resolution","1920*1080"]
[null,null,"Contrast","5000:1（Typ.) (Transmission)"]
[]
[null,"Touch screen","Touch technology","Non-contact infrared sensing technology"]
[null,null,"Induction objects","Opaque objects(as finger,pen,etc.)"]
[null,null,"Touch pressure","Zero"]
[null,null,"Multi-point support","2 points, 4 points,10 points"]
[null,null,"Touch screen glass"," 4mm, physical toughened Morse 7 grade explosion-proof,"]
[{"$nulls":3},"light transmittance>95%"]
[null,null,"Operating system","Support Win7, WinXP, Win2000, Linux, etc"]
[]
[null,"Android system","Chip","4cores RK3188"]
[null,null,"Memory","2G"]
[null,null,"Internal memory","8G, extendable"]
[null,null,"Video card","Android HD"]
[null,null,"Operating system","Android 4.2.2"]
[null,null,"Kernal version","3.0.28"]
[null,null,"Input power supply","220V AC 50/60HZ"]